// C++ code

//

void setup()

{

Serial.begin(9600);

pinMode(8, OUTPUT);

pinMode(9, OUTPUT);

pinMode(10, OUTPUT);

pinMode(11, OUTPUT);

pinMode(12, OUTPUT);

}

void loop()

{

digitalWrite(8, HIGH);

delay(100);

digitalWrite(9, HIGH);

delay(100);

digitalWrite(10, HIGH);

delay(100);

digitalWrite(11, HIGH);

delay(100);

digitalWrite(12, HIGH);

delay(100);

digitalWrite(8, LOW);

delay(100);

digitalWrite(9, LOW);

delay(100);

digitalWrite(10, LOW);

delay(100);

digitalWrite(11, LOW);

delay(100);

digitalWrite(12, LOW);

delay(100);

}